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UÇAK VE HELİKOPTER İÇİN PRATİK DENEYİM KAYIT DEFTERİ

HBL-66 Hava Aracı Bakım Lisansı Pratik Deneyim Defteri Kapak Sayfası
 





	Adı Soyadı
	
	Doğum Tarihi
	

	Kimlik/Pasaport Numarası
	
	Doğum Yeri
	





Bu deneyim defterinde sunmakta olduğum bilgilerin tam ve doğru olduğunu beyan eder, verdiğim bilgilerin doğru çıkmaması halinde HBL-66 Hava Aracı Bakım Lisansı alamayacağımı ve hakkımda idari yaptırım uygulanabileceğini kabul ederim.


	İmzası
	


  












UÇAK VE HELİKOPTER İÇİN PRATİK DENEYİM KAYIT DEFTERİ

Pratik Deneyim Kayıt Defterinin Doldurulma Usul ve Esasları
 
1. Bu kayıt defterinin amacı, hava aracı bakım lisansına pratik deneyim ile tip veya tam (alt) grup ilavesi amacıyla operasyondaki hava araçları üzerindeki bakım deneyimini belgelemektir. Örneğin; B1.2 kategori lisansa, pratik deneyim ile hava aracı tip ilavesi yapılması.
2. Defterde kayıt altına alınan bakım deneyimleri, tutulan bakım kayıtları üzerinden ispat edilebilir olmalıdır.
3. Bir bakım taskı farklı bölümlere ayrılamaz. İlgili bakım taskının uygulanması aşamasında birden fazla işlem türü gerçekleştiriliyorsa tek bir bakım kaydı olarak deftere kaydedilir. 
4. Lisans kategorisine, hava aracı tipine ve hava aracı (alt) grup yetkilerine uygun olarak defterde bulunan her bölümden bakım tecrübesi sunulmalıdır. 
5. Pratik deneyim gösterilecek hava aracı tipine ve hava aracı (alt) grup yetkileri için efektif olmayan bölümler N/A olarak işaretlenebilecektir. Örneğin pratik deneyim kaydı sunulan hava aracı tipinde ATA chapter 18 bulunmadığı durumlarda ilgili bölüm değerlendirme dışında tutulacak olup defterde N/A olarak işaretlenebilecektir.
6. Efektif olmayan bölümler N/A olarak işaretlendikten sonra kalan her bölümde belirlenen tasklardan en az 1 adet deneyim gösterilmesi zorunlu olmakla beraber; her bölümde yer alan task sayısının en az yarısı kadar sayıda deneyim gösterilmelidir. Örneğin; ATA chapter 5 için toplam task sayısı 8 olarak belirlenmiştir. 3 adet mevcut tasklardan gerçekleştirilmişse ilave olarak Chapter 5’ten en az 1 task eklenmelidir.
7. İlave edilen tasklarda mümkün olduğunca işlem çeşitliliği sağlanır. (R/I, FOT, SGH gibi)
8. İlave edilecek bakım taskları her bölümün sonunda ‘Additional Items’ kısmına kaydedilecektir. ‘Additional Items’ kısmına ilave satır eklenerek daha fazla deneyim gösterilebilir. İlave edilen task sayıları sonuç tablosunda bulunan ‘İlave Edilen Task Sayısı’ sütununa kaydedilir.
9. Sonuç tablosu bütün parametreleri içerecek şekilde eksiksiz olarak doldurulacaktır. Eksik doldurulan satırlar değerlendirmeye alınmayacaktır.
10. Pratik Deneyim bir bakım kuruluşunda edinilmiş ise deneyim defterinin, deneyimin kazanıldığı bakım kuruluşunun bakım ve uyumluluk izleme birimleri tarafından incelenerek, bahse konu işlemler ile bakım kuruluşu kayıtlarının uyumlu olduğuna dair onaylanması gerekmektedir. 
11. Bağımsız onaylayıcı personel gözetiminde gerçekleştirilen kayıtlar için ise kayıtların uyumlu olduğuna dair bağımsız onaylayıcı personel tarafından onaylanması gerekmektedir.
12. Bir bakım taskı, lisansında yer alan başka bir kategori veya başka bir lisansına bağlı yetkilendirmesi kapsamında başvuranın kendisi tarafından yapılabiliyorsa, ilgili task için Süpervizör Onayı hanesi kendisi tarafından imzalanır.
13. Genel Müdürlüğün sunulan kayıtların uygunluğu vb. nedenler ile doğrulama hakkı saklıdır. İlgili kayıtların doğruluğu, imzası bulunan kişilerin sorumluluğundadır.

R/I: Removal / Installation, FOT: Functional / Operational Test, SGH: Service and Ground Handling, INSP: Inspection, MEL: Minimum Equipment List, TS: Trouble Shooting


         
	No
	ATA
Ch.
	Task Tanımı
	R / I
	FOT
	SGH
	INSP
	Tarih
(DD.MM.YY)
	İş Emri
	Task Card 
veya Logbook referansı.
	Hava Aracı
Tipi
	Tescil
İşareti
	Süpervizör
Mühür ve İmza

	TIME LIMITS/MAINTENANCE CHECKS

	1
	
	100 hour check (general aviation aircraft).
	
	
	
	
	
	
	
	
	
	

	2
	
	‘B’ or ‘C’ check (transport category aircraft).
	
	
	
	
	
	
	
	
	
	

	3
	
	Assist carrying out a scheduled maintenance check i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	4
	
	Review Aircraft maintenance log for correct completion.
	
	
	
	
	
	
	
	
	
	

	5
	
	Review records for compliance with Airworthiness Directives.
	
	
	
	
	
	
	
	
	
	

	6
	
	Review records for compliance with component life limits.
	
	
	
	
	
	
	
	
	
	

	7
	
	Procedure for inspection following heavy landing.
	
	
	
	
	
	
	
	
	
	

	8
	
	Procedure for inspection following lightning strike.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TIME LIMITS/MAINTENANCE CHECKS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	DIMENSIONS/AREAS

	1
	
	Locate component(s) by zone/station number.
	
	
	
	
	
	
	
	
	
	

	2
	
	Perform symmetry check.
	
	
	
	
	
	
	
	
	
	

	LIFTING AND SHORING

	
	
	Assist in:
	
	
	
	
	
	
	
	
	
	

	1
	
	Jack aircraft nose or tail wheel.
	
	
	
	
	
	
	
	
	
	

	2
	
	Jack complete aircraft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Sling or trestle major component.
	
	
	
	
	
	
	
	
	
	

	Additional Items for LIFTING AND SHORING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	LEVELLING/WEIGHING

	1
	
	Level aircraft.
	
	
	
	
	
	
	
	
	
	

	2
	
	Weigh aircraft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Prepare weight and balance amendment.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check aircraft against equipment list.
	
	
	
	
	
	
	
	
	
	

	Additional Items for LEVELLING/WEIGHING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	TOWING AND TAXIING

	1
	
	Prepare for aircraft towing.
	
	
	
	
	
	
	
	
	
	

	2
	
	Tow aircraft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Be part of aircraft towing team.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TOWING AND TAXIING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	PARKING AND MOORING

	1
	
	Tie down aircraft.
	
	
	
	
	
	
	
	
	
	

	2
	
	Park, secure and cover aircraft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Position aircraft in dock.
	
	
	
	
	
	
	
	
	
	

	4
	
	Secure rotor blades.
	
	
	
	
	
	
	
	
	
	

	Additional Items for PARKING AND MOORING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	PLACARDS AND MARKINGS

	1
	
	Check aircraft for correct placards.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check aircraft for correct markings.
	
	
	
	
	
	
	
	
	
	

	SERVICING

	1
	
	Refuel aircraft.
	
	
	
	
	
	
	
	
	
	

	2
	
	Defuel aircraft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Carry out tank to tank fuel transfer.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check/adjust tire pressures.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check/replenish oil level.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check/replenish hydraulic fluid level.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check/replenish accumulator pressure.
	
	
	
	
	
	
	
	
	
	

	8
	
	Charge pneumatic system.
	
	
	
	
	
	
	
	
	
	

	SERVICING

	9
	
	Grease aircraft.
	
	
	
	
	
	
	
	
	
	

	10
	
	Connect ground power.
	
	
	
	
	
	
	
	
	
	

	11
	
	Service toilet/water system
	
	
	
	
	
	
	
	
	
	

	12
	
	Perform pre-flight/daily check.
	
	
	
	
	
	
	
	
	
	

	Additional Items for SERVICING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	VIBRATION AND NOISE ANALYSIS (ONLY HELICOPTER)

	1
	
	Analyse helicopter vibration problem.
	
	
	
	
	
	
	
	
	
	

	2
	
	Analyse noise spectrum.
	
	
	
	
	
	
	
	
	
	

	3
	
	Analyse engine vibration.
	
	
	
	
	
	
	
	
	
	

	Additional Items for VIBRATION AND NOISE ANALYSIS (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	AIR CONDITIONING

	1
	
	Replace combustion heater.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace flow control valve.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace outflow valve.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace safety valve.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace vapour cycle unit.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace air cycle unit.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace cabin blower.
	
	
	
	
	
	
	
	
	
	

	8
	
	Replace heat exchanger.
	
	
	
	
	
	
	
	
	
	

	9
	
	Replace pressurisation controller.
	
	
	
	
	
	
	
	
	
	

	10
	
	Clean outflow valves.
	
	
	
	
	
	
	
	
	
	

	11
	
	Deactivate/reactivate cargo isolation valve.
	
	
	
	
	
	
	
	
	
	

	AIR CONDITIONING

	12
	
	Deactivate/reactivate avionics ventilation components.
	
	
	
	
	
	
	
	
	
	

	13
	
	Check operation of air conditioning/heating system.
	
	
	
	
	
	
	
	
	
	

	14
	
	Check operation of pressurisation system.
	
	
	
	
	
	
	
	
	
	

	15
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for AIR CONDITIONING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	
	
	
	
	
	

	AUTO FLIGHT

	1
	
	Install servos.
	
	
	
	
	
	
	
	
	
	

	2
	
	Rig bridle cables Replace controller.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace amplifier.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replacement of the auto flight system LRUs in case of fly-by-wire aircraft.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check operation of auto-pilot.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check operation of auto-throttle/auto-thrust.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check operation of yaw damper.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check and adjust servo clutch.
	
	
	
	
	
	
	
	
	
	

	9
	
	Perform autopilot gain adjustments.
	
	
	
	
	
	
	
	
	
	

	10
	
	Perform mach trim functional check.
	
	
	
	
	
	
	
	
	
	

	11
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	12
	
	Check autoland system.
	
	
	
	
	
	
	
	
	
	

	13
	
	Check flight management systems.
	
	
	
	
	
	
	
	
	
	

	14
	
	Check stability augmentation system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for AUTO FLIGHT

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	COMMUNICATIONS

	1
	
	Replace VHF COM unit.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace HF COM unit.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace existing antenna.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace static discharge wicks.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check operation of radios.
	
	
	
	
	
	
	
	
	
	

	6
	
	Perform antenna VSWR check.
	
	
	
	
	
	
	
	
	
	

	COMMUNICATIONS

	7
	
	Perform SELCAL operational check.
	
	
	
	
	
	
	
	
	
	

	8
	
	Perform operational check of passenger address system.
	
	
	
	
	
	
	
	
	
	

	9
	
	Functionally check audio integrating system.
	
	
	
	
	
	
	
	
	
	

	10
	
	Repair coaxial cable.
	
	
	
	
	
	
	
	
	
	

	11
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	12
	
	Check SATCOM.
	
	
	
	
	
	
	
	
	
	

	Additional Items for COMMUNICATIONS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	ELECTRICAL POWER

	1
	
	Charge lead/acid battery.
	
	
	
	
	
	
	
	
	
	

	2
	
	Charge Ni-Cad battery.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check battery capacity.
	
	
	
	
	
	
	
	
	
	

	4
	
	Deep-cycle Ni-Cad battery.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace integrated drive/generator/alternator.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace switches.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace circuit breakers.
	
	
	
	
	
	
	
	
	
	

	8
	
	Adjust voltage regulator.
	
	
	
	
	
	
	
	
	
	

	9
	
	Change voltage regulator.
	
	
	
	
	
	
	
	
	
	

	10
	
	Amend electrical load analysis report.
	
	
	
	
	
	
	
	
	
	

	11
	
	Repair/replace electrical feeder cable.
	
	
	
	
	
	
	
	
	
	

	12
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Electrical Power

	13
	
	Perform functional check of integrated drive/generator/alternator.
	
	
	
	
	
	
	
	
	
	

	14
	
	Perform functional check of voltage regulator.
	
	
	
	
	
	
	
	
	
	

	15
	
	Perform functional check of emergency generation system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ELECTRICAL POWER

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	
	
	
	
	
	

	EQUIPMENT/FURNISHINGS

	1
	
	Replace carpets
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace crew seats.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace passenger seats.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check inertia reels.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check seats/belts for security.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check emergency equipment.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check ELT for compliance with regulations.
	
	
	
	
	
	
	
	
	
	

	8
	
	Repair toilet waste container.
	
	
	
	
	
	
	
	
	
	

	9
	
	Remove and install ceiling and sidewall panels.
	
	
	
	
	
	
	
	
	
	

	10
	
	Repair upholstery.
	
	
	
	
	
	
	
	
	
	

	11
	
	Change cabin configuration.
	
	
	
	
	
	
	
	
	
	

	12
	
	Replace cargo loading system actuator.
	
	
	
	
	
	
	
	
	
	

	13
	
	Test cargo loading system.
	
	
	
	
	
	
	
	
	
	

	14
	
	Replace escape slides/ropes.
	
	
	
	
	
	
	
	
	
	

	Additional Items for EQUIPMENT/FURNISHINGS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	FIRE PROTECTION

	1
	
	Check fire bottle contents.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check/test operation of fire/smoke detection and warning system.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check cabin fire extinguisher contents.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check lavatory smoke detector system.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check cargo panel sealing.
	
	
	
	
	
	
	
	
	
	

	6
	
	Install new fire bottle.
	
	
	
	
	
	
	
	
	
	

	FIRE PROTECTION

	7
	
	Replace fire bottle squib.
	
	
	
	
	
	
	
	
	
	

	8
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	9
	
	Inspect engine fire wire detection systems.
	
	
	
	
	
	
	
	
	
	

	Additional Items for FIRE PROTECTION

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	FLIGHT CONTROLS

	1
	
	Inspect primary flight controls and related components i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	2
	
	Extending/retracting flaps & slats.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace horizontal stabiliser.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace spoiler/lift damper.
	
	
	
	
	
	
	
	
	
	

	FLIGHT CONTROLS

	5
	
	Replace elevator.
	
	
	
	
	
	
	
	
	
	

	6
	
	Deactivation/reactivation of aileron servo control.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace aileron.
	
	
	
	
	
	
	
	
	
	

	8
	
	Replace rudder.
	
	
	
	
	
	
	
	
	
	

	9
	
	Replace trim tabs.
	
	
	
	
	
	
	
	
	
	

	10
	
	Install control cable and fittings.
	
	
	
	
	
	
	
	
	
	

	11
	
	Replace slats.
	
	
	
	
	
	
	
	
	
	

	12
	
	Replace flaps.
	
	
	
	
	
	
	
	
	
	

	13
	
	Replace powered flying control unit.
	
	
	
	
	
	
	
	
	
	

	14
	
	Replace flat actuator.
	
	
	
	
	
	
	
	
	
	

	15
	
	Rig primary flight controls.
	
	
	
	
	
	
	
	
	
	

	16
	
	Adjust trim tab.
	
	
	
	
	
	
	
	
	
	

	17
	
	Adjust control cable tension.
	
	
	
	
	
	
	
	
	
	

	FLIGHT CONTROLS

	18
	
	Check control range and direction of movement.
	
	
	
	
	
	
	
	
	
	

	19
	
	Check for correct assembly and locking.
	
	
	
	
	
	
	
	
	
	

	20
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	21
	
	Functional test of primary flight controls.
	
	
	
	
	
	
	
	
	
	

	22
	
	Functional test of flap system.
	
	
	
	
	
	
	
	
	
	

	23
	
	Operational test of the side stick assembly.
	
	
	
	
	
	
	
	
	
	

	24
	
	Operational test of the THS.
	
	
	
	
	
	
	
	
	
	

	25
	
	THS system wear check.
	
	
	
	
	
	
	
	
	
	

	Additional Items for FLIGHT CONTROLS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	Additional Items for FLIGHT CONTROLS

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	
	
	
	
	
	

	8
	
	
	
	
	
	
	
	
	
	
	
	

	9
	
	
	
	
	
	
	
	
	
	
	
	

	10
	
	
	
	
	
	
	
	
	
	
	
	

	11
	
	
	
	
	
	
	
	
	
	
	
	

	12
	
	
	
	
	
	
	
	
	
	
	
	

	FUEL

	1
	
	Water drain system (operation).
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace booster pump.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace fuel selector.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace fuel tank cells.
	
	
	
	
	
	
	
	
	
	

	FUEL

	5
	
	Replace/test fuel control valves.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace magnetic fuel level indicators.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace water drain valve.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check/calculate fuel contents manually.
	
	
	
	
	
	
	
	
	
	

	9
	
	Check filters.
	
	
	
	
	
	
	
	
	
	

	10
	
	Flow check system.
	
	
	
	
	
	
	
	
	
	

	11
	
	Check calibration of fuel quantity gauges.
	
	
	
	
	
	
	
	
	
	

	12
	
	Check operation feed/selectors.
	
	
	
	
	
	
	
	
	
	

	13
	
	Check operation of fuel dump/jettison system.
	
	
	
	
	
	
	
	
	
	

	14
	
	Fuel transfer between tanks.
	
	
	
	
	
	
	
	
	
	

	15
	
	Pressure defuel.
	
	
	
	
	
	
	
	
	
	

	16
	
	Pressure refuel (manual control).
	
	
	
	
	
	
	
	
	
	

	17
	
	Deactivation/reactivation of the fuel valves (transfer defuel, X-feed, refuel).
	
	
	
	
	
	
	
	
	
	

	18
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for FUEL

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	
	
	
	
	
	

	8
	
	
	
	
	
	
	
	
	
	
	
	

	HYDRAULICS

	1
	
	Replace engine driven pump.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check/replace case drain filter.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace standby pump.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace hydraulic motor pump/generator.
	
	
	
	
	
	
	
	
	
	

	HYDRAULICS

	5
	
	Replace accumulator.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check operation of shut off valve.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check filters/clog indicators.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check indicating systems.
	
	
	
	
	
	
	
	
	
	

	9
	
	Perform functional checks.
	
	
	
	
	
	
	
	
	
	

	10
	
	Pressurisation/depressurisation of the hydraulic system.
	
	
	
	
	
	
	
	
	
	

	11
	
	Power Transfer Unit (PTU) operation.
	
	
	
	
	
	
	
	
	
	

	12
	
	Replacement of PTU.
	
	
	
	
	
	
	
	
	
	

	13
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for HYDRAULICS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	Additional Items for HYDRAULICS

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	ICE AND RAIN PROTECTION

	1
	
	Replace pump.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace timer.
	
	
	
	
	
	
	
	
	
	

	3
	
	Inspect repair propeller deice boot.
	
	
	
	
	
	
	
	
	
	

	4
	
	Test propeller de-icing system.
	
	
	
	
	
	
	
	
	
	

	5
	
	Inspect/test wing leading edge de-icer boot.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace anti-ice/deice valve.
	
	
	
	
	
	
	
	
	
	

	7
	
	Install wiper motor.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check operation of systems.
	
	
	
	
	
	
	
	
	
	

	9
	
	Operational test of the pitot-probe ice protection.
	
	
	
	
	
	
	
	
	
	

	ICE AND RAIN PROTECTION

	10
	
	Operational test of the TAT ice protection.
	
	
	
	
	
	
	
	
	
	

	11
	
	Operational test of the wing ice protection system.
	
	
	
	
	
	
	
	
	
	

	12
	
	Assistance to the operational test of the engine air-intake ice protection (with engines operating).
	
	
	
	
	
	
	
	
	
	

	13
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ICE AND RAIN PROTECTION

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	INDICATING/RECORDING SYSTEMS

	1
	
	Replace flight data recorder.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace cockpit voice recorder.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace clock.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace master caution unit.
	
	
	
	
	
	
	
	
	
	

	5
	
	Perform FDR data retrieval.
	
	
	
	
	
	
	
	
	
	

	6
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	7
	
	Implement ESDS procedures.
	
	
	
	
	
	
	
	
	
	

	8
	
	Inspect for HIRF requirements.
	
	
	
	
	
	
	
	
	
	

	9
	
	Start/stop EIS procedure.
	
	
	
	
	
	
	
	
	
	

	10
	
	Bite test of the CFDIU.
	
	
	
	
	
	
	
	
	
	

	11
	
	Ground scanning of the central warning system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for INDICATING/RECORDING SYSTEMS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	LANDING GEAR

	1
	
	Build up wheel.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace main wheel.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace nose wheel.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace steering actuator.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace truck tilt actuator.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace gear retraction actuator.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace uplock/downlock assembly.
	
	
	
	
	
	
	
	
	
	

	LANDING GEAR

	8
	
	Replace shimmy damper.
	
	
	
	
	
	
	
	
	
	

	9
	
	Rig nose wheel steering.
	
	
	
	
	
	
	
	
	
	

	10
	
	Functional test of the nose wheel steering system.
	
	
	
	
	
	
	
	
	
	

	11
	
	Replace shock strut seals.
	
	
	
	
	
	
	
	
	
	

	12
	
	Replace brake unit.
	
	
	
	
	
	
	
	
	
	

	13
	
	Replace brake control valve.
	
	
	
	
	
	
	
	
	
	

	14
	
	Bleed brakes.
	
	
	
	
	
	
	
	
	
	

	15
	
	Replace brake fan.
	
	
	
	
	
	
	
	
	
	

	16
	
	Test anti-skid unit.
	
	
	
	
	
	
	
	
	
	

	17
	
	Test gear retraction.
	
	
	
	
	
	
	
	
	
	

	18
	
	Change bungees.
	
	
	
	
	
	
	
	
	
	

	19
	
	Adjust micro switches/sensors.
	
	
	
	
	
	
	
	
	
	

	20
	
	Charge struts with oil and air.
	
	
	
	
	
	
	
	
	
	

	LANDING GEAR

	21
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	22
	
	Test auto-brake system.
	
	
	
	
	
	
	
	
	
	

	23
	
	Replace rotorcraft skids.
	
	
	
	
	
	
	
	
	
	

	24
	
	Replace rotorcraft skid shoes.
	
	
	
	
	
	
	
	
	
	

	25
	
	Pack and check floats.
	
	
	
	
	
	
	
	
	
	

	26
	
	Flotation equipment.
	
	
	
	
	
	
	
	
	
	

	27
	
	Check/test emergency blowdown (emergency landing gear extension).
	
	
	
	
	
	
	
	
	
	

	28
	
	Operational test of the landing gear doors.
	
	
	
	
	
	
	
	
	
	

	Additional Items for LANDING GEAR

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	
	
	
	
	
	

	8
	
	
	
	
	
	
	
	
	
	
	
	

	9
	
	
	
	
	
	
	
	
	
	
	
	

	10
	
	
	
	
	
	
	
	
	
	
	
	

	11
	
	
	
	
	
	
	
	
	
	
	
	

	12
	
	
	
	
	
	
	
	
	
	
	
	

	13
	
	
	
	
	
	
	
	
	
	
	
	

	LIGHTS

	1
	
	Repair/replace rotating beacon.
	
	
	
	
	
	
	
	
	
	

	2
	
	Repair/replace landing lights.
	
	
	
	
	
	
	
	
	
	

	3
	
	Repair/replace navigation lights.
	
	
	
	
	
	
	
	
	
	

	4
	
	Repair/replace interior lights.
	
	
	
	
	
	
	
	
	
	

	LIGHTS

	5
	
	Replace ice inspection lights.
	
	
	
	
	
	
	
	
	
	

	6
	
	Repair/replace logo lights.
	
	
	
	
	
	
	
	
	
	

	7
	
	Repair/replace emergency lighting system.
	
	
	
	
	
	
	
	
	
	

	8
	
	Perform emergency lighting system checks.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system
	
	
	
	
	
	
	
	
	
	

	Additional Items for LIGHTS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	INSTRUMENTS

	1
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	2
	
	Calibrate magnetic direction indicator.
	
	
	
	
	
	
	
	
	
	

	INSTRUMENTS

	3
	
	Replace airspeed indicator.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace altimeter.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace air-data computer.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace ADI.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace HSI.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check pitot static system for leaks.
	
	
	
	
	
	
	
	
	
	

	9
	
	Check operation of directional gyro.
	
	
	
	
	
	
	
	
	
	

	10
	
	Check calibration of pitot static instruments.
	
	
	
	
	
	
	
	
	
	

	11
	
	Compass replacement direct/indirect.
	
	
	
	
	
	
	
	
	
	

	12
	
	Functional check flight director system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for INSTRUMENTS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	SURVEILLANCE 

	1
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	2
	
	Functional check weather radar.
	
	
	
	
	
	
	
	
	
	

	3
	
	Functional check doppler.
	
	
	
	
	
	
	
	
	
	

	4
	
	Functional check TCAS.
	
	
	
	
	
	
	
	
	
	

	5
	
	Functional check ATC transponder.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check calibration of pressure altitude reporting system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for SURVEILLANCE

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	NAVIGATION

	1
	
	Functional check inertial navigation system.
	
	
	
	
	
	
	
	
	
	

	2
	
	Complete quadrantal error correction of ADF system.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check GPS.
	
	
	
	
	
	
	
	
	
	

	4
	
	Test AVM.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check marker systems.
	
	
	
	
	
	
	
	
	
	

	6
	
	Functional check DME.
	
	
	
	
	
	
	
	
	
	

	Additional Items for NAVIGATION

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	OXYGEN

	1
	
	Inspect on board oxygen equipment.
	
	
	
	
	
	
	
	
	
	

	2
	
	Purge and recharge oxygen system.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace regulator.
	
	
	
	
	
	
	
	
	
	

	OXYGEN

	4
	
	Replace oxygen generator.
	
	
	
	
	
	
	
	
	
	

	5
	
	Test crew oxygen system.
	
	
	
	
	
	
	
	
	
	

	6
	
	Perform auto oxygen system deployment check.
	
	
	
	
	
	
	
	
	
	

	7
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for OXYGEN

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	PNEUMATIC SYSTEMS

	1
	
	Replace filter.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace air shut off valve.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace pressure regulating valve.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace compressor.
	
	
	
	
	
	
	
	
	
	

	PNEUMATIC SYSTEMS

	5
	
	Recharge dessicator.
	
	
	
	
	
	
	
	
	
	

	6
	
	Adjust regulator.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check for leaks.
	
	
	
	
	
	
	
	
	
	

	8
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for PNEUMATIC SYSTEMS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	VACUUM SYSTEMS

	1
	
	Inspect the vacuum system i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace vacuum pump.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check/replace filters.
	
	
	
	
	
	
	
	
	
	

	4
	
	Adjust regulator.
	
	
	
	
	
	
	
	
	
	

	5
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for VACUUM SYSTEMS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	WATER/WASTE

	1
	
	Replace water pump.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace tap.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace toilet pump.
	
	
	
	
	
	
	
	
	
	

	4
	
	Perform water heater functional check.
	
	
	
	
	
	
	
	
	
	

	5
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	6
	
	Inspect waste bin flap closure.
	
	
	
	
	
	
	
	
	
	

	Additional Items for WATER/WASTE

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	CENTRAL MAINTENANCE SYSTEM

	1
	
	Retrieve data from CMU.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace CMU.
	
	
	
	
	
	
	
	
	
	

	3
	
	Perform Bite check.
	
	
	
	
	
	
	
	
	
	

	4
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for CENTRAL MAINTENANCE SYSTEM

	1
	
	
	
	
	
	
	
	
	
	
	
	

	AIRBORNE AUXILIARY POWER

	1
	
	Install APU.
	
	
	
	
	
	
	
	
	
	

	2
	
	Inspect hot section.
	
	
	
	
	
	
	
	
	
	

	3
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for AIRBORNE AUXILIARY POWER

	1
	
	
	
	
	
	
	
	
	
	
	
	

	STRUCTURES

	1
	
	Assessment of damage.
	
	
	
	
	
	
	
	
	
	

	2
	
	Sheet metal repair.
	
	
	
	
	
	
	
	
	
	

	3
	
	Fibre glass repair.
	
	
	
	
	
	
	
	
	
	

	4
	
	Wooden repair.
	
	
	
	
	
	
	
	
	
	

	5
	
	Fabric repair.
	
	
	
	
	
	
	
	
	
	

	6
	
	Recover fabric control surface.
	
	
	
	
	
	
	
	
	
	

	7
	
	Treat corrosion.
	
	
	
	
	
	
	
	
	
	

	8
	
	Apply protective treatment.
	
	
	
	
	
	
	
	
	
	

	Additional Items for STRUCTURES

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	DOORS

	1
	
	Inspect passenger door i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	2
	
	Rig/adjust locking mechanism.
	
	
	
	
	
	
	
	
	
	

	3
	
	Adjust air stair system.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check operation of emergency exits.
	
	
	
	
	
	
	
	
	
	

	5
	
	Test door warning system.
	
	
	
	
	
	
	
	
	
	

	6
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	7
	
	Remove and install passenger door i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	8
	
	Remove and install emergency exit i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	9
	
	Inspect cargo door i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	Additional Items for DOORS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	WINDOWS

	1
	
	Replace windshield.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace direct vision window.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace cabin window.
	
	
	
	
	
	
	
	
	
	

	4
	
	Repair transparency.
	
	
	
	
	
	
	
	
	
	

	Additional Items for WINDOWS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	WINGS

	1
	
	Skin repair.
	
	
	
	
	
	
	
	
	
	

	2
	
	Recover fabric wing.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace tip.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace rib.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace integral fuel tank panel.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check incidence/rig.
	
	
	
	
	
	
	
	
	
	

	Additional Items for WINGS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	PROPELLER

	1
	
	Assemble prop after transportation.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace propeller.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace governor.
	
	
	
	
	
	
	
	
	
	

	4
	
	Adjust governor.
	
	
	
	
	
	
	
	
	
	

	5
	
	Perform static functional checks.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check operation during ground run.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check track.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check setting of micro switches.
	
	
	
	
	
	
	
	
	
	

	9
	
	Assessment of blade damage i.a.w. AMM.
	
	
	
	
	
	
	
	
	
	

	10
	
	Dynamically balance prop.
	
	
	
	
	
	
	
	
	
	

	11
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for PROPELLER

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	
	
	
	
	
	

	MAIN ROTORS (ONLY HELICOPTER)

	1
	
	Install rotor assembly.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace blades.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace damper assembly.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check track.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check static balance.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check dynamic balance.
	
	
	
	
	
	
	
	
	
	

	7
	
	Troubleshoot.
	
	
	
	
	
	
	
	
	
	

	Additional Items for MAIN ROTORS (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	ROTOR DRIVE (ONLY HELICOPTER)

	1
	
	Replace mast.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace drive coupling.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace clutch/freewheel unit
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace drive belt.
	
	
	
	
	
	
	
	
	
	

	5
	
	Install main gearbox.
	
	
	
	
	
	
	
	
	
	

	6
	
	Overhaul main gearbox.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check gearbox chip detectors.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ROTOR DRIVE (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	TAIL ROTORS (ONLY HELICOPTER)

	1
	
	Install rotor assembly.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace blades.
	
	
	
	
	
	
	
	
	
	

	3
	
	Troubleshoot.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TAIL ROTORS (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	TAIL ROTOR DRIVE (ONLY HELICOPTER)

	1
	
	Replace bevel gearbox.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace universal joints.
	
	
	
	
	
	
	
	
	
	

	3
	
	Overhaul bevel gearbox.
	
	
	
	
	
	
	
	
	
	

	4
	
	Install drive assembly.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check chip detectors.
	
	
	
	
	
	
	
	
	
	

	6
	
	Check/install bearings and hangers.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check/service/assemble flexible couplings.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check alignment of drive shafts.
	
	
	
	
	
	
	
	
	
	

	9
	
	Install and rig drive shafts.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TAIL ROTOR DRIVE (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	ROTORCRAFT FLIGHT CONTROLS (ONLY HELICOPTER)

	1
	
	Install swash plate.
	
	
	
	
	
	
	
	
	
	

	2
	
	Install mixing box.
	
	
	
	
	
	
	
	
	
	

	3
	
	Adjust pitch links.
	
	
	
	
	
	
	
	
	
	

	4
	
	Rig collective system.
	
	
	
	
	
	
	
	
	
	

	5
	
	Rig cyclic system.
	
	
	
	
	
	
	
	
	
	

	6
	
	Rig anti-torque system.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check controls for assembly and locking.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check controls for operation and sense.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TAIL ROTOR DRIVE (ONLY HELICOPTER)

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	POWER PLANT

	1
	
	Build up ECU.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace engine.
	
	
	
	
	
	
	
	
	
	

	3
	
	Repair cooling baffles.
	
	
	
	
	
	
	
	
	
	

	4
	
	Repair cowling.
	
	
	
	
	
	
	
	
	
	

	5
	
	Adjust cowl flaps.
	
	
	
	
	
	
	
	
	
	

	6
	
	Repair faulty wiring.
	
	
	
	
	
	
	
	
	
	

	7
	
	Troubleshoot.
	
	
	
	
	
	
	
	
	
	

	8
	
	Assist in dry motoring check.
	
	
	
	
	
	
	
	
	
	

	9
	
	Assist in wet motoring check.
	
	
	
	
	
	
	
	
	
	

	10
	
	Assist in engine start (manual mode).
	
	
	
	
	
	
	
	
	
	

	Additional Items for POWER PLANT

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	PISTON ENGINES

	1
	
	Remove/install reduction gear.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check crankshaft run-out.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check tappet clearance.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check compression.
	
	
	
	
	
	
	
	
	
	

	5
	
	Extract broken stud.
	
	
	
	
	
	
	
	
	
	

	6
	
	Install helicoil.
	
	
	
	
	
	
	
	
	
	

	7
	
	Perform ground run.
	
	
	
	
	
	
	
	
	
	

	8
	
	Establish/check reference RPM.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot.
	
	
	
	
	
	
	
	
	
	

	Additional Items for PISTON ENGINES

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	TURBINE ENGINES

	1
	
	Replace module.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace fan blade.
	
	
	
	
	
	
	
	
	
	

	3
	
	Hot section inspection/boroscope check.
	
	
	
	
	
	
	
	
	
	

	4
	
	Carry out engine/compressor wash.
	
	
	
	
	
	
	
	
	
	

	5
	
	Carry out engine dry cycle.
	
	
	
	
	
	
	
	
	
	

	6
	
	Engine ground run.
	
	
	
	
	
	
	
	
	
	

	7
	
	Establish reference power.
	
	
	
	
	
	
	
	
	
	

	8
	
	Trend monitoring/gas path analysis.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TURBINE ENGINES

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	FUEL AND CONTROL, PISTON

	1
	
	Replace engine driven pump.
	
	
	
	
	
	
	
	
	
	

	2
	
	Adjust AMC.
	
	
	
	
	
	
	
	
	
	

	3
	
	Adjust ABC.
	
	
	
	
	
	
	
	
	
	

	4
	
	Install carburettor/injector.
	
	
	
	
	
	
	
	
	
	

	5
	
	Adjust carburettor/injector.
	
	
	
	
	
	
	
	
	
	

	6
	
	Clean injector nozzles.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace primer line.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check carburettor float setting.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for FUEL AND CONTROL, PISTON

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	FUEL AND CONTROL, TURBINE

	1
	
	Replace FCU.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace Engine Electronic Control Unit (FADEC).
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace Fuel Metering Unit (FADEC).
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace engine driven pump.
	
	
	
	
	
	
	
	
	
	

	5
	
	Clean/test fuel nozzles.
	
	
	
	
	
	
	
	
	
	

	6
	
	Clean/replace filters.
	
	
	
	
	
	
	
	
	
	

	7
	
	Adjust FCU.
	
	
	
	
	
	
	
	
	
	

	8
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	9
	
	Functional test of FADEC.
	
	
	
	
	
	
	
	
	
	

	Additional Items for FUEL AND CONTROL, TURBINE

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	IGNITION SYSTEMS, PISTON

	1
	
	Change magneto.
	
	
	
	
	
	
	
	
	
	

	2
	
	Change ignition vibrator.
	
	
	
	
	
	
	
	
	
	

	3
	
	Change plugs.
	
	
	
	
	
	
	
	
	
	

	4
	
	Test plugs.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check H.T. leads.
	
	
	
	
	
	
	
	
	
	

	6
	
	Install new leads.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check timing.
	
	
	
	
	
	
	
	
	
	

	8
	
	Check system bonding.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for IGNITION SYSTEMS, PISTON

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	IGNITION SYSTEMS, TURBINE

	1
	
	Perform functional test of the ignition system.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check glow plugs/ignitors.
	
	
	
	
	
	
	
	
	
	

	3
	
	Check H.T. leads.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check ignition unit.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace ignition unit.
	
	
	
	
	
	
	
	
	
	

	6
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for IGNITION SYSTEMS, TURBINE

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	ENGINE CONTROLS

	1
	
	Rig thrust lever.
	
	
	
	
	
	
	
	
	
	

	2
	
	Rig RPM control.
	
	
	
	
	
	
	
	
	
	

	3
	
	Rig mixture HP cock lever.
	
	
	
	
	
	
	
	
	
	

	4
	
	Rig power lever.
	
	
	
	
	
	
	
	
	
	

	5
	
	Check control sync (multi-eng).
	
	
	
	
	
	
	
	
	
	

	6
	
	Check controls for correct assembly and locking.
	
	
	
	
	
	
	
	
	
	

	7
	
	Check controls for range and direction of movement.
	
	
	
	
	
	
	
	
	
	

	8
	
	Adjust pedestal micro-switches.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ENGINE CONTROLS

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	ENGINE INDICATING

	1
	
	Replace engine instruments(s).
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace oil temperature bulb.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace thermocouples.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check calibration.
	
	
	
	
	
	
	
	
	
	

	5
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ENGINE INDICATING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	EXHAUST, PISTON

	1
	
	Replace exhaust gasket.
	
	
	
	
	
	
	
	
	
	

	2
	
	Inspect welded repair.
	
	
	
	
	
	
	
	
	
	

	3
	
	Pressure check cabin heater muff.
	
	
	
	
	
	
	
	
	
	

	4
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for EXHAUST, PISTON

	1
	
	
	
	
	
	
	
	
	
	
	
	

	EXHAUST, TURBINE

	1
	
	Change jet pipe.
	
	
	
	
	
	
	
	
	
	

	2
	
	Change shroud assembly.
	
	
	
	
	
	
	
	
	
	

	3
	
	Install trimmers.
	
	
	
	
	
	
	
	
	
	

	4
	
	Inspect/replace thrust reverser.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace thrust reverser component.
	
	
	
	
	
	
	
	
	
	

	6
	
	Deactivate/reactivate thrust reverser.
	
	
	
	
	
	
	
	
	
	

	7
	
	Operational test of the thrust reverser system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for EXHAUST, TURBINE

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	OIL

	1
	
	Change oil.
	
	
	
	
	
	
	
	
	
	

	2
	
	Check filter(s).
	
	
	
	
	
	
	
	
	
	

	3
	
	Adjust pressure relief valve.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace oil tank.
	
	
	
	
	
	
	
	
	
	

	5
	
	Replace oil pump.
	
	
	
	
	
	
	
	
	
	

	6
	
	Replace oil cooler.
	
	
	
	
	
	
	
	
	
	

	7
	
	Replace firewall shut off valve.
	
	
	
	
	
	
	
	
	
	

	8
	
	Perform oil dilution test.
	
	
	
	
	
	
	
	
	
	

	9
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for OIL

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	
	
	
	
	
	

	STARTING

	1
	
	Replace starter.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace start relay.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace start control valve.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check cranking speed.
	
	
	
	
	
	
	
	
	
	

	5
	
	Troubleshoot faulty system.
	
	
	
	
	
	
	
	
	
	

	Additional Items for STARTING

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	TURBINES, PISTON ENGINES

	1
	
	Replace PRT.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace turbo-blower.
	
	
	
	
	
	
	
	
	
	

	3
	
	Replace heat shields.
	
	
	
	
	
	
	
	
	
	

	4
	
	Replace waste gate.
	
	
	
	
	
	
	
	
	
	

	5
	
	Adjust density controller.
	
	
	
	
	
	
	
	
	
	

	Additional Items for TURBINES, PISTON ENGINES

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	ENGINE WATER INJECTION

	1
	
	Replace water/methanol pump.
	
	
	
	
	
	
	
	
	
	

	2
	
	Flow check water/methanol system.
	
	
	
	
	
	
	
	
	
	

	3
	
	Adjust water/methanol control unit.
	
	
	
	
	
	
	
	
	
	

	4
	
	Check fluid for quality.
	
	
	
	
	
	
	
	
	
	

	5
	
	Troubleshoot faulty system
	
	
	
	
	
	
	
	
	
	

	Additional Items for ENGINE WATER INJECTION

	1
	
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	
	

	ACCESSORY GEAR BOXES

	1
	
	Replace gearbox.
	
	
	
	
	
	
	
	
	
	

	2
	
	Replace drive shaft.
	
	
	
	
	
	
	
	
	
	

	3
	
	Inspect magnetic chip detector.
	
	
	
	
	
	
	
	
	
	

	Additional Items for ACCESSORY GEAR BOXES

	1
	
	
	
	
	
	
	
	
	
	
	
	

	APU

	1
	
	Removal/installation of the APU.
	
	
	
	
	
	
	
	
	
	

	2
	
	Removal/installation of the inlet guide-vane actuator.
	
	
	
	
	
	
	
	
	
	

	3
	
	Operational test of the APU emergency shut-down test.
	
	
	
	
	
	
	
	
	
	

	4
	
	Operational test of the APU.
	
	
	
	
	
	
	
	
	
	

	Additional Items for APU

	1
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